**List all Part Number and/or Components Required:**

|  |  |
| --- | --- |
| **Part Number** | **Description** |
| 2316 | CleanView Swivel Pet |
| 23169 | CleanView Swivel Pet NWD |
| 1614760 | 23169 Kraft Carton |
| 1631488 | Dirt Tank POP |
| 1631490 | Foot POP |
| 1631489 | Side Talker POP |
| 1633180 | Blackstock Sticker |
| 1633181 | DCPI Sticker |
| 1633187 | UPC Sticker |

**Instructions:**

1. Remove unit 2316 from the original carton

1. Cut prongs off the cord (to create a non-working display)
2. Secure/glue tools on the vacuum

1. Place Tank POP (1631488) in center of the tank

1. Take the plastic clip and peel off the adhesive cover and stick it to the right side of the vacuum tank. Slide Side Talker POP (1631489) into the plastic clip


  

1. Take another plastic clip and peel off the adhesive cover and stick it to the left side of the vacuum foot. Slide Foot Talker POP (1631489) into the plastic clip




1. Once all previous steps are completed, the fully assembled display should look like this: 
2. Place the unit into the kraft carton (1614760) and tape closed.
3. Place Backstock Sticker (Part #1633180) on all four side panels. This can be placed anywhere on the side panel as long as it it not covering any text.



1. Place DPCI Sticker (Part #1633181) on all four side panels. This can be placed anywhere on the side panel as long as it it not covering any text.



1. Place UPC Sticker (Part #1633187) on all four side panels. This can be placed anywhere on the side panel as long as it it not covering any text.

