**List all Part Number and/or Components Required:**

|  |  |
| --- | --- |
| **Part Number** | **Description** |
| 3437 | CleanView Compact Turbo |
| 1644342 | Carton, Kraft - NWD CleanView Compact Turbo NWD - 3761 |
| 1631146 | POP, Tank Sticker, CleanView Compact Turbo, 34363 |
| 1631144 | POP, Side Talker, CleanView Compact Turbo, 34363 |
|  |  |

 **Instructions:**



1. Ensure 625 units are ordered of model 3437 to the Elwood DC for Meijer & Fred Meyer conversion
	1. 275 for Meijer
	2. 350 for Fred Meyer
2. Remove 3437 from the litho carton & assemble product
3. Remove prongs on the cord



1. secure/glue tools on the vacuum
	1. TubroBrush Tool, Crevice Tool, Dusting Brush Tool



1. Remove PRL label and Add NWD UPC sticker on the back of the unit – Label PN: 1644604



1. Add POP sticker to front of dirty tank as shown in example picture – POP PN: 1631146



1. Adding POP side talker to Right of tank w/NWD adhesive clips or side talker adhesive - POP PN: 1631144







1. Printing/utilizing NEW NWD Kraft Carton 1644342 (not part of current model 34363)
	1. Will need to print locally from Green Bay Packaging and ship to Elwood DC
2. Adding green carton Labels from Sales (Cassie Pfahler to provide to DC)
3. We will **NOT** be needing the Lowe’s reset stickers provided on the product matrix
4. ~~(1637242,1637240)~~ as we are using this Lowe’s model for the Meijer reset
5. Place FULLY ASSEMBLED unit into 1 of the cartons provided by Green Bay
6. Bubble Wrap unit and conceal unit by taping bubble wrap
7. Place unit into carton
8. Fill voids inside carton with buddle wrap
9. Tape carton shut
10. Place units on pallet according to 34363 pallet instructions on Supplier Site.