**List all Part Number and/or Components Required:**

|  |  |
| --- | --- |
| **Part Number** | **Description** |
| 25542 | CrossWave® Cordless Max Litho Carton |
| Model #2554A & UPC: 011120248838 | Warehouse to print stickers and place on cartons |
| 1625325 | Amazon transparency Label |
|  |  |
|  |  |

 **Instructions:**

1. Get a 25542 unit (Litho Carton)
2. Add the new model # 2554A and UPC 011120248838 stickers to the back of the carton, per image below.
	1. Be sure all stickers are covering up the current model # 25542 & UPC



1. Add Amazon Transparency Label (**Part 1625325**)
	1. Unique Amazon Transparency Labels to be printed by supplier and sent to DC
	2. When applying the Transparency label, allow a minimum of .25” (7mm) between the edge of the label and the edge of the packaging.
	3. If placing the Transparency label on the same side/plane as another bar code (UPC, EAN, etc) use a minimum spacing of 1.75” (45mm). If placing above another code, spacing should be minimum of .25” (7mm).
	4. Place the Transparency content in a location that is clearly visible and easily accessible to scan.
2. Repalletize completed unit per the pallet diagram for item 2554A on supplier.bissell.com